Revision History / Thinkbook Plus G2 Huaqin (System box)

Rev.a 2020.10.13
 Initial Release
 SCheckCapG14T_v0.02.0
 wflash_g14t_3_26(32)
 FW v0001rev03 (5299, 529B)
       v0001rev10 (5298)
 
Rev.b 2020.10.27
 Initial Release
 SCheckCapG14T_v0.02.3 support for home key for Thinkbook Plus G2
 wflash_g14t_3_26(32)
 FW v0001rev03 (5299, 529B)
       v0001rev13 (5298)

Rev.c 2020.11.17
 FW v0001rev15 (5298)
 Changed : CAL_THRESHOLD=975 (5298)
 Changed : CALTH_IGNORELINE=1,1,2,1 (5298)
 Changed : LUT (5298)
 Add batch file.
 Execute these files and start SCheckCap automatically. 
 
Rev.d 2020.11.18
 SCheckCapG14T_v0.02.3k
 Changed : VID=0x048D (5298)
 Changed : PID=0x8957 (5298)

Rev.e 2020.11.20
 Update .bat file.
 Add chkhidpid

Rev.f 2020.12.16
 FW v0001rev16 (5298)

Rev.g 2020.12.24
 FW v0001rev20 (5298)
        v0001rev04 (5299, 529B)
  Changed : RAW_INPUT=1 (5299)
 Changed : LUT (5298)
 Changed : HK_TOUCH=2100 (5298)

Rev.h 2021.3.5
 [PID5298]
 FW v0001rev24
 Changed : RAW_INPUT=1
 Disabled : RAW_INPUT_REGISTOR
 Changed : CAL_THRESHOLD=292
 Changed : HK_TOUCH=2000
 Changed : TIPC_TPS=7
 Changed : X, Y LUT

 [PID5299, 529B]
 FW v0002rev00
 Changed : RAW_INPUT=0
 Changed : RAW_INPUT_REGISTOR=5
 Changed : AES_LOG_ONLY=0
 Changed : TIPC_TPS=7

Rev.i 2021.3.18
 FW v0002rev02 (529B)
 Changed : CAL_THRESHOLD=292 (529B)
 
Rev.j 2021.3.24
 FW v0002rev07 (5298)
 Changed : RAW_INPUT=0 (5298)
 Changed : RAW_INPUT_REGISTOR=5 (5298)
 Changed : AES_LOG_ONLY=0 (5298)
 Changed : HK_TOUCH=300
 Disabled : HK_REMOVE=, HK_REMOVE_LOW=
 
Rev.k 2021.4.10
 FW v0002rev12 (5298)
 Changed : HK_TOUCH=200
 
Rev.l 2021.4.16
 FW v0002rev13 (5298)
 Changed : HK_TOUCH=250 (5298)
 
Rev.m 2021.4.23
 SCheckCapG14T_v0.02.6m
 [PID5299]
 FW v0002rev02
	 Chenged : RAW_INPUT_REGISTOR=20
	 Changed : CAL_THRESHOLD=292
 [PID5298]
	 Added : HOMEKEY2_CHECK=0
	           HK2_TOUCH_TIMEOUT=10000
	           HK2_REMOVE_TIMEOUT=10000
	           ;HK2_TOUCH_TH_HIGH=500
	           HK2_TOUCH_TH_LOW=225
	           HK2_REMOVE_TH_HIGH=170
	           ;HK2_REMOVE_TH_LOW=0
	           HK2_DATA_COUNT=16 

Rev.n 2021.4.23
 SCheckCapG14T_v0.02.7m

Rev.o 2021.5.12
 ScheckCapG14T_v0.02.8m	
 [PID5298]
	FW v0002rev14
	Changed: HK bit = 0 by default in maintenance mode
 