Release Notification
*******************************************************************************
Rw EEPROM information.                                               21/SEP/2018
ControlWosEEPROM.exe

Version: 1.0.0.1 

Fixed/Modification:
            First Edit (#15015)

USAGE : ControlWosEEPROM.exe [/r|/w|/?] [Bank] [Start_Addr] [End_Addr] [Hex string/[ASCII string]] [/e ENV_string]
        /r              Read data from EEPROM.
        /e              Write data that read from EEPROM into specific (ENV_string).cmd file for set environment variable.
        /w              Write data into EEPROM and Double check it.
        /?              Show help information.
        Bank            Bank of EEPROM: 0~7 (hexadecimal data).
        Start_Addr      Start address: 0~ff (hexadecimal data).
        End_Addr        End address  : 0~ff (hexadecimal data).
        Hex string      Hex string for write EEPROM, two character combine to one data.
                        Ex: 6162636465
        ASCII string    ASCII string for write EEPROM, one character is equal one data.
                        Ex: [abcde]
        ENV_string      ENV_string for write environment variable, English word.
                        Ex: USER
Example:
            ControlWosEEPROM.exe /?
If you want to set environment variable from EEPROM data.
            ControlWosEEPROM.exe /r 0 A0 A5 /e USER
If you want to write MAC (00-1B-77-02-77-BC) into EEPROM(Bank 0,offset A0h~A5h):
            ControlWosEEPROM.exe /w 0 A0 A5 001B770277BC

Return Value:           
        0: FAIL
        1: SUCCESS

Note:
1. Support WOS project only 
2. PJT.bin is required.
*******************************************************************************